# Hummingbird HW design NOTE!!!

1. When connect to RF chip by SPI, need use SCK, MISO, MOSI, SS together.

MCU takes as master